|  |
| --- |
| Municipal Pool Facility Hazard Identification Inspection |
| Agency: | Inspection Date: |
| Name of Inspector: | Title: |
| Location Inspected: |
| # | Needs Work | OK | N/A | Condition Surveyed  |
|  | Signage |
| 1 |  |  |  | Load rating for pool posted? |
| 2 |  |  |  | All pool rules and restrictions are posted? i.e. no alcohol |
| 3 |  |  |  | Is the UV burn index forecast posted daily? |
|  | Life Guard Stand  |
| 4 |  |  |  | One elevated lifeguard chair is required for each 3,400 ft2of pool surface |
| 5 |  |  |  | A complete spine board with all necessary ties? |
| 6 |  |  |  | A unit of lifesaving equipment provided for each 2,000 ft2 of water surface area |
| 7 |  |  |  | A rescue tube or rescue buoy at each pool lifeguard station? |
| 8 |  |  |  | Suction break E-Switch installed and labeled?  |
| 9 |  |  |  | All lifeguards have a loud whistle to alert bathers?  |
| 10 |  |  |  | Lifeguards wear hats, sunglasses and sunscreen? Shade provided? |
|  | Wading Pools |
| 11 |  |  |  | Separate filtration system and turnover rate? |
| 12 |  |  |  | Physical barrier separating it from other pools? |
|  | Diving Boards/ Sliding Boards |
| 13 |  |  |  | Instruction signs and rules posted near the device? |
| 14 |  |  |  | Boards have slip-resistant tread surfaces? Slides have running water?  |
| 15 |  |  |  | Steps & ladders lead to diving boards with handrails to water edge? |
|  | Pool Depth Markings |
| **16** |  |  |  | Depth markings are displayed at pool edge & top surface every 25 feet? |
| **17** |  |  |  | Depth markings placed at Max & Min points |
| **18** |  |  |  | Markings must be minimum 4 inches high in a contrasting color? |
|  | Written Plans to Guide Lifeguard Actions |
| 19 |  |  |  | Copy of NJAC 8:26 available to Pool management? |
| 20 |  |  |  | A written aquatics supervision plan is available to all lifeguards? |
| 21 |  |  |  | A written Emergency Plan is available to all lifeguards? |
| 22 |  |  |  | Facility has a written lightning response plan |
|  | Chlorine/ Disinfection Treatment Areas |
| 23 |  |  |  | Identification signs posted? |
| 24 |  |  |  | Pool makeup water protected by a backflow prevention device? |
| 25 |  |  |  | Automatic disinfectant leak detector & alarm installed? |
| 26 |  |  |  | Safety Shower /eye wash within 25 feet? |
| 27 |  |  |  | Is the Bonding & Grounding certificate posted as required by NJ Law S213? |
| 28 |  |  |  | Is pool provided with an automatic means of adding a disinfectant? |
|  | Locker Rooms |
| 29 |  |  |  | Slip resistant floors throughout? |
| 30 |  |  |  | Electrical fixtures rated for wet areas? All receptacles GFCI protected? |
| 31 |  |  |  | Natural or mechanical ventilation provides minimum of 2 air changes/hour? |
| Exterior Post lamps |
| 32 |  |  |  | Inspect exterior pole lamp posts for cracks in welds |