|  |
| --- |
| Fitness/Exercise RoomFacilities Hazard Identification Inspection |
| Agency: | Inspection Date: |
| Name of Inspector: | Title: |
| Location Inspected: |
| # | Needs Work | N/A | OK | Condition Surveyed |
|  | Facility |
| 1 |  |  |  | Tile flooring resistant to slips |
| 2 |  |  |  | Rubber flooring free of slits, cuts and large gaps between pieces |
| 3 |  |  |  | Carpet free of tears |
| 4 |  |  |  | Flooring glued or fastened down properly with no trip hazards  |
| 5 |  |  |  | Mirrors placed 20” or greater off of the floor |
| 6 |  |  |  | Mirrors are not damaged or cracked (replace immediately if damaged) |
| 7 |  |  |  | Ceiling tiles are present and not damaged |
| 8 |  |  |  | Ceiling height sufficient for overhead exercises |
| 9 |  |  |  | Egress pathways kept clear |
| 10 |  |  |  | Sufficient lighting |
|  | Exercise Equipment |
| 11 |  |  |  | Mats and upholstery free of tears and cracks |
| 12 |  |  |  | Equipment properly stored after use and returned to avoid pathway obstruction |
| 13 |  |  |  | Easy access to equipment |
| 14 |  |  |  | Area free of loose bolts, screws, chains and cables |
| 15 |  |  |  | No protruding screws or parts that need tightening or removal |
| 16 |  |  |  | Parts and surfaces properly lubricated and cleaned |
| 17 |  |  |  | Belts, chains and cables aligned with machine parts |
| 18 |  |  |  | No worn parts visible (chains, belts, cables, bolts, cracked joints, etc.) |
| 19 |  |  |  | Protective padding free of cracks and tears |
| 20 |  |  |  | Benches and weight racks are secured to the floor or wall |
| 21 |  |  |  | Remove or place sign on damaged equipment |
|  | Cleaning |
| 22 |  |  |  | Clean all flooring |
| 24 |  |  |  | Clean and disinfect upholstery |
| 25 |  |  |  | Clean and disinfect drinking fountain |
| 26 |  |  |  | Clean and disinfect surfaces that contact skin |
| 27 |  |  |  | Remove trash and garbage |
| 28 |  |  |  | Ensure equipment is returned and stored properly |
| 29 |  |  |  | Clean rust from equipment with rust-removing solution |
| 30 |  |  |  | Replace lightbulbs as needed |