**Hydraulic Floor & Bottle Jacks Inspection Checklist**

|  |  |  |  |
| --- | --- | --- | --- |
| Agency | Location | Date | Inspector |

**Procedure:**

* Look for any cracks, dents, or other signs of damage to the housing, pump assembly, and other components.
* Check for any signs of hydraulic fluid leaks, especially around seals, connections, and the pump.
* Ensure the hydraulic fluid is at the correct level, and that the fill plug is secure.
* Raise an appropriate load and hold it for several minutes to check for leaks or malfunctions. Check for slow or uneven lifting, leaks, load drooping, or no lift at all.

🞏 Bottle jack 🞏Floor jack Jack ID: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Capacity: \_\_\_\_\_\_\_\_

|  |  |  |  |
| --- | --- | --- | --- |
| **Condition** | **Pass** | **Fail** | **N/A** |
| The rated load capacity is legible and permanently stamped or otherwise marked. |  |  |  |
| All operating and warning are labels legible. |  |  |  |
| The stop indicator is clean and visible to determine the limit of travel. |  |  |  |
| The jack is adequately lubricated and moving parts travel freely. |  |  |  |
| There is no visible damage to base, body, or lifting mechanism. |  |  |  |
| There is no sign of leaking hydraulic fluid or failing hydraulic seals. |  |  |  |

🞏 Bottle jack 🞏Floor jack Jack ID: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Capacity: \_\_\_\_\_\_\_\_

|  |  |  |  |
| --- | --- | --- | --- |
| **Condition** | **Pass** | **Fail** | **N/A** |
| The rated load capacity is legible and permanently stamped or otherwise marked. |  |  |  |
| All operating and warning are labels legible. |  |  |  |
| The stop indicator is clean and visible to determine the limit of travel. |  |  |  |
| The jack is adequately lubricated and moving parts travel freely. |  |  |  |
| There is no visible damage to base, body, or lifting mechanism. |  |  |  |
| There is no sign of leaking hydraulic fluid or failing hydraulic seals. |  |  |  |

🞏 Bottle jack 🞏Floor jack Jack ID: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Capacity: \_\_\_\_\_\_\_\_

|  |  |  |  |
| --- | --- | --- | --- |
| **Condition** | **Pass** | **Fail** | **N/A** |
| The rated load capacity is legible and permanently stamped or otherwise marked. |  |  |  |
| All operating and warning are labels legible. |  |  |  |
| The stop indicator is clean and visible to determine the limit of travel. |  |  |  |
| The jack is adequately lubricated and moving parts travel freely. |  |  |  |
| There is no visible damage to base, body, or lifting mechanism. |  |  |  |
| There is no sign of leaking hydraulic fluid or failing hydraulic seals. |  |  |  |

🞏 Bottle jack 🞏Floor jack Jack ID: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Capacity: \_\_\_\_\_\_\_\_

|  |  |  |  |
| --- | --- | --- | --- |
| **Condition** | **Pass** | **Fail** | **N/A** |
| The rated load capacity is legible and permanently stamped or otherwise marked. |  |  |  |
| All operating and warning are labels legible. |  |  |  |
| The stop indicator is clean and visible to determine the limit of travel. |  |  |  |
| The jack is adequately lubricated and moving parts travel freely. |  |  |  |
| There is no visible damage to base, body, or lifting mechanism. |  |  |  |
| There is no sign of leaking hydraulic fluid or failing hydraulic seals. |  |  |  |