|  |
| --- |
| Facility Hazard Identification Inspections – Public Pool |
| Agency: | Pool Name: |
| Name of Inspector: | Inspection Date: |
| # | Needs Work | OK | N/A | Condition Surveyed  |
|  | Signage |
| 1 |  |  |  | Load rating, rules and restrictions for pool are posted? |
| 2 |  |  |  | Is the UV burn index forecast posted daily?  |
|  | Main Pool  |
| 3 |  |  |  | One elevated lifeguard chair is required for each 3,400 ft2 of pool surface |
| 4 |  |  |  | A complete spine board with all necessary ties? |
| 5 |  |  |  | A unit of lifesaving equipment provided for each 2,000 ft2 of water surface area? |
| 6 |  |  |  | A rescue tube or rescue buoy at each pool lifeguard station? |
| 7 |  |  |  | Sufficient number of USCG-approved personal flotation devices are available? |
| 8 |  |  |  | Suction break E-Switch installed and labeled?  |
| 9 |  |  |  | All lifeguards have a loud whistle to alert bathers?  |
| 10 |  |  |  | Lifeguards wear hats, sunglasses and sunscreen? Shade provided? |
| 11 |  |  |  | 4-inch high depth markings are displayed on pool edge & top surface at maximum & minimum points, and every 25 feet? |
|  | Wading Pools |
| 12 |  |  |  | Separate filtration system and turnover rate? |
| 13 |  |  |  | Physical barrier separating it from other pools? |
|  | Diving Boards/ Sliding Boards |
| 14 |  |  |  | Instruction signs and rules posted near the device? |
| 15 |  |  |  | Boards have slip-resistant tread surfaces? Slides have running water?  |
| 16 |  |  |  | Steps & ladders lead to diving boards with handrails to water edge? |
|  | Written Plans to Guide Lifeguard Actions |
| 17 |  |  |  | Copy of NJAC 8:26 available to Pool management? |
| 18 |  |  |  | A written aquatics supervision plan is available to all lifeguards? |
| 19 |  |  |  | A written Emergency Plan is available to all lifeguards? |
| 20 |  |  |  | Facility has a written lightning response plan |
|  | Chlorine/ Disinfection Treatment Areas |
| 21 |  |  |  | Identification signs posted? |
| 22 |  |  |  | Pool makeup water protected by a backflow prevention device? |
| 23 |  |  |  | Automatic disinfectant leak detector & alarm installed? |
| 24 |  |  |  | Safety shower /eye wash within 25 feet? |
| 25 |  |  |  | Is the bonding & grounding certificate posted as required by NJ Law S-213? |
| 26 |  |  |  | Is pool provided with an automatic means of adding a disinfectant? |
|  | Locker Rooms |
| 27 |  |  |  | Slip resistant floors throughout? |
| 28 |  |  |  | Electrical fixtures rated for wet areas? All receptacles are GFCI protected? |
| 29 |  |  |  | Natural or mechanical ventilation provides minimum of 2 air changes/hour? |
|  | Exterior Post lamps |
| 30 |  |  |  | Inspect exterior pole lamp posts inspected for cracks in welds |