|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Facility Hazard Identification Inspections – Public Pool | | | | | | |
| Agency: | | | | | | Pool Name: |
| Name of Inspector: | | | | | | Inspection Date: |
| # | Needs  Work | OK | N/A | | Condition Surveyed | |
|  | Signage | | | | | |
| 1 |  |  |  | | Load rating, rules and restrictions for pool are posted? | |
| 2 |  |  |  | | Is the UV burn index forecast posted daily? | |
|  | Main Pool | | | | | |
| 3 |  |  |  | | One elevated lifeguard chair is required for each 3,400 ft2 of pool surface | |
| 4 |  |  |  | | A complete spine board with all necessary ties? | |
| 5 |  |  |  | | A unit of lifesaving equipment provided for each 2,000 ft2 of water surface area? | |
| 6 |  |  |  | | A rescue tube or rescue buoy at each pool lifeguard station? | |
| 7 |  |  |  | | Sufficient number of USCG-approved personal flotation devices are available? | |
| 8 |  |  |  | | Suction break E-Switch installed and labeled? | |
| 9 |  |  |  | | All lifeguards have a loud whistle to alert bathers? | |
| 10 |  |  |  | | Lifeguards wear hats, sunglasses and sunscreen? Shade provided? | |
| 11 |  |  |  | | 4-inch high depth markings are displayed on pool edge & top surface at maximum &  minimum points, and every 25 feet? | |
|  | Wading Pools | | | | | |
| 12 |  |  |  | | Separate filtration system and turnover rate? | |
| 13 |  |  |  | | Physical barrier separating it from other pools? | |
|  | Diving Boards/ Sliding Boards | | | | | |
| 14 |  |  |  | | Instruction signs and rules posted near the device? | |
| 15 |  |  |  | | Boards have slip-resistant tread surfaces? Slides have running water? | |
| 16 |  |  |  | | Steps & ladders lead to diving boards with handrails to water edge? | |
|  | Written Plans to Guide Lifeguard Actions | | | | | |
| 17 |  |  |  | | Copy of NJAC 8:26 available to Pool management? | |
| 18 |  |  |  | | A written aquatics supervision plan is available to all lifeguards? | |
| 19 |  |  |  | | A written Emergency Plan is available to all lifeguards? | |
| 20 |  |  |  | | Facility has a written lightning response plan | |
|  | Chlorine/ Disinfection Treatment Areas | | | | | |
| 21 |  |  |  | | Identification signs posted? | |
| 22 |  |  |  | | Pool makeup water protected by a backflow prevention device? | |
| 23 |  |  |  | | Automatic disinfectant leak detector & alarm installed? | |
| 24 |  |  |  | | Safety shower /eye wash within 25 feet? | |
| 25 |  |  |  | | Is the bonding & grounding certificate posted as required by NJ Law S-213? | |
| 26 |  |  |  | | Is pool provided with an automatic means of adding a disinfectant? | |
|  | Locker Rooms | | | | | |
| 27 |  |  |  | Slip resistant floors throughout? | | |
| 28 |  |  |  | Electrical fixtures rated for wet areas? All receptacles are GFCI protected? | | |
| 29 |  |  |  | Natural or mechanical ventilation provides minimum of 2 air changes/hour? | | |
|  | Exterior Post lamps | | | | | |
| 30 |  |  |  | Inspect exterior pole lamp posts inspected for cracks in welds | | |