BLEACHER & GRANDSTAND INSPECTION CHECKLIST
	Facility Name:
	____________________________
	Location / Address:
	____________________________

	Bleacher ID / Unit #:
	____________________________
	Bleacher Type:
	____________________________

	Number of Rows:
	____________________________
	Inspection Date:
	____________________________

	Inspector Name:
	____________________________
	Inspection Type:
	____________________________

	Weather Conditions:
	____________________________
	Last Inspection Date:
	____________________________


Bleacher Type: Permanent / Portable / Telescopic / Temporary     |     Inspection Type: Pre-Season / Mid-Season / Post-Season / Post-Storm / Routine
SECTION 1: STRUCTURAL INTEGRITY
	Inspection Item
	Pass
	Fail
	N/A
	Comments

	No loose or missing hardware on cross-braces and frame connections
	☐
	☐
	☐
	

	No cracked or broken welds
	☐
	☐
	☐
	

	Bleacher is solidly anchored or attached to ground surface
	☐
	☐
	☐
	

	No bent or warped benches or components
	☐
	☐
	☐
	

	No sharp edges from damage
	☐
	☐
	☐
	

	No missing or damaged safety end caps
	☐
	☐
	☐
	

	No rust or signs of significant corrosion
	☐
	☐
	☐
	

	No signs of environmental stress damage (rot, UV degradation, etc.)
	☐
	☐
	☐
	

	Identification tag present with installation and inspection information
	☐
	☐
	☐
	

	Structural condition acceptable (no signs of imminent failure or collapse risk)
	☐
	☐
	☐
	



SECTION 2: GUARDRAILS & FALL PROTECTION
	Inspection Item
	Pass
	Fail
	N/A
	Comments

	Guardrails present on backs and open ends where footboard/seatboard/aisle is 30 inches or more above ground
	☐
	☐
	☐
	

	Guardrail top surface is at least 42 inches above leading edge of footboard, seatboard, or aisle
	☐
	☐
	☐
	

	All guardrail openings prevent passage of a 4-inch diameter sphere (up to 34 inches height)
	☐
	☐
	☐
	

	Openings between 34 and 42 inches height prevent passage of an 8-inch diameter sphere
	☐
	☐
	☐
	

	Guardrail infill uses vertical members only; no ladder-like patterns
	☐
	☐
	☐
	

	Any foothold openings in guardrail infill are no wider than 1.75 inches
	☐
	☐
	☐
	

	If chain-link fencing used: mesh size is 1.25 inches square or smaller
	☐
	☐
	☐
	

	Guardrails are free of damage, bending, or looseness
	☐
	☐
	☐
	

	Where bleachers are adjacent to a wall: 4-inch sphere cannot pass between bleachers and wall
	☐
	☐
	☐
	




SECTION 3: SEATING COMPONENT OPENINGS
	Inspection Item
	Pass
	Fail
	N/A
	Comments

	Openings between footboard and seatboard prevent passage of a 4-inch diameter sphere (where 30+ inches above grade)
	☐
	☐
	☐
	

	Openings between seatboard and riser prevent passage of a 4-inch diameter sphere (where 30+ inches above grade)
	☐
	☐
	☐
	

	No openings that would permit a fall of 30 inches or more
	☐
	☐
	☐
	

	Aisle accessways more than 30 inches above grade: openings prevent passage of a 4-inch diameter sphere
	☐
	☐
	☐
	

	Horizontal gaps between footboards and seatboards do not exceed 0.25 inch
	☐
	☐
	☐
	



SECTION 4: EGRESS & ACCESSIBILITY
	Inspection Item
	Pass
	Fail
	N/A
	Comments

	Aisles are clear of obstructions
	☐
	☐
	☐
	

	Minimum aisle width is maintained per applicable standards
	☐
	☐
	☐
	

	Stepped aisle tread depth is at least 11 inches
	☐
	☐
	☐
	

	Stepped aisle riser height is between 4 and 8 inches
	☐
	☐
	☐
	

	Tread and riser dimensions are uniform throughout (tolerance ≤ 0.375 inch)
	☐
	☐
	☐
	

	Row-to-row spacing is at least 22 inches
	☐
	☐
	☐
	

	Minimum seat depth is 9 inches
	☐
	☐
	☐
	

	For exterior installations: travel distance from any seat to perimeter does not exceed 400 feet
	☐
	☐
	☐
	

	Exit signage is visible and in good condition (where applicable)
	☐
	☐
	☐
	

	Accessible routes and seating areas are unobstructed
	☐
	☐
	☐
	



SECTION 5: HANDRAILS
	Inspection Item
	Pass
	Fail
	N/A
	Comments

	Handrails present on all required stepped aisles
	☐
	☐
	☐
	

	Handrail height is 34 to 38 inches above tread nosings
	☐
	☐
	☐
	

	Mid-aisle handrails are discontinuous at intervals not exceeding 5 rows
	☐
	☐
	☐
	

	Gaps in mid-aisle handrails are between 22 and 36 inches wide
	☐
	☐
	☐
	

	Handrail gripping surfaces are continuous and free of obstructions
	☐
	☐
	☐
	

	Handrails are free of sharp or abrasive elements
	☐
	☐
	☐
	

	Clear space between handrail and wall/surface is at least 1.5 inches
	☐
	☐
	☐
	

	Handrails are structurally sound and firmly attached
	☐
	☐
	☐
	





SECTION 6: CAPACITY & SIGNAGE
	Inspection Item
	Pass
	Fail
	N/A
	Comments

	Maximum occupancy/load capacity is posted on the bleacher unit
	☐
	☐
	☐
	

	Identification tag is present and legible (includes installation and inspection info)
	☐
	☐
	☐
	

	Any required warning notices are posted (for units not yet certified as compliant)
	☐
	☐
	☐
	

	No visible overcrowding or overloading conditions
	☐
	☐
	☐
	



SECTION 7: PORTABLE / TEMPORARY BLEACHERS  (Complete if applicable)
	Inspection Item
	Pass
	Fail
	N/A
	Comments

	Bleacher is set up on stable, level ground
	☐
	☐
	☐
	

	Anchoring and stabilization confirmed per manufacturer specifications
	☐
	☐
	☐
	

	No damage from transport or previous setup/breakdown cycles
	☐
	☐
	☐
	

	Manufacturer's rated capacity is not exceeded
	☐
	☐
	☐
	

	Setup verified by trained personnel prior to use
	☐
	☐
	☐
	



SECTION 8: OVERALL ASSESSMENT
	Overall Condition Rating:
	☐ Satisfactory     ☐ Requires Monitoring     ☐ Requires Repair Before Next Use     ☐ Remove from Service Immediately

	Bleacher Approved for Use:
	☐ Yes     ☐ No

	If No — Date Closed/Tagged Out:
	___________________________



DEFICIENCIES NOTED
Complete for each deficiency identified. Attach additional sheets if needed.
	Item
#
	Description of Deficiency
	Location on
Structure
	Severity
(L/M/H)
	Corrective Action
Required
	Assigned
To
	Target
Completion
	Date
Resolved

	1
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	

	7
	
	
	
	
	
	
	

	8
	
	
	
	
	
	
	

	9
	
	
	
	
	
	
	

	10
	
	
	
	
	
	
	




INSPECTOR CERTIFICATION
"I certify that this inspection was conducted in accordance with applicable standards and that the findings recorded above are accurate to the best of my knowledge."
	Inspector Signature:
	______________________________
	Date:
	______________________________

	Print Name:
	______________________________
	Title:
	______________________________

	Supervisor Review (if required):
	______________________________
	Date:
	______________________________



NOTES / ADDITIONAL OBSERVATIONS
______________________________________________________________________________________________________________
______________________________________________________________________________________________________________
______________________________________________________________________________________________________________
______________________________________________________________________________________________________________
______________________________________________________________________________________________________________
______________________________________________________________________________________________________________

REFERENCES
New Jersey Standard on Bleachers, Folding and Telescopic Seating, and Grandstands 2017 (N.J.A.C. 5:23), based on ICC 300-2017
CPSC Guidelines for Retrofitting Bleachers
ICC 300-2017: Standard for Bleachers, Folding and Telescopic Seating, and Grandstands

