|  |
| --- |
| Recreation DepartmentFacilities Hazard Identification Inspection |
| Agency: | Inspection Date: |
| Name of Inspector: | Title: |
| Location Inspected: |
| # | Needs Work | N/A | OK | Condition Surveyed |
|  | Soccer Fields |
| 1 |  |  |  | Are goal cages anchored or weighted to prevent tipping |
| 2 |  |  |  | Are team benches, if provided, at least 10 feet from field edge |
| 3 |  |  |  | First aid and BBP kits available and contents inspected regularly |
|  | Baseball Field |
| 4 |  |  |  | If dugouts are provided, is full frontal foul ball protection in place |
| 5 |  |  |  | If town is member of *Little League International* are break-away bases used |
| 6 |  |  |  | Is bat and helmet storage provided, check for impalement hazards on racks |
| 7 |  |  |  | Are batting cages and warm-up pitcher areas fully enclosed, including top |
| 8 |  |  |  | Walked the field looking for holes and debris? |
| 9 |  |  |  | Are outfield fences if 4’ or less covered with “roll-over” protection on the top |
| 10 |  |  |  | Are field usage rules posted – i.e., no alcohol or glass bottles |
|  | Sports Equipment Storage Areas |
| 11 |  |  |  | Are storage buildings & roof are structurally sound |
| 12 |  |  |  | Are doors secured & in good condition, any broken windows |
| 13 |  |  |  | Any signs of vandalism |
| 14 |  |  |  | Are interiors seasonally inspected, cleaned & no hazardous material storage i.e., gasoline |
|  | Sports Equipment Storage Areas |
| 15 |  |  |  | Are entrance and exit pads in good condition and free of obstructions |
| 16 |  |  |  | Are trash receptacles and smoker ash trays provided outside |
| 17 |  |  |  | Are doors secured or open 24/7. Informational signs in place |
| 18 |  |  |  | Is exterior lighting provided? Is it operational? Lights on timer or photo cell? |
|  | Parking Areas and Paths |
| 19 |  |  |  | Are there sufficient parking spots for the intended occupancy of the facility |
| 20 |  |  |  | Is recreation facility patrolled by local police |
| 21 |  |  |  | Are wheel stops or guard rails provided at the field sides of the lot |
| 22 |  |  |  | If lighting is provided, is it adequate and does it cover all lot areas & access roads |
| 24 |  |  |  | Are vehicle bridges provided over gullies and streams equipped with guard rails |
| 25 |  |  |  | Are pedestrian bridges in good repair and provided with guard and hand rails |
| 26 |  |  |  | If benches are provided are they in good repair and in designated spots |
| 27 |  |  |  | Are paths restricted to walkers or open to joggers, rollerblades or bikes. Any concerns? |
| 28 |  |  |  | Are improved (paved) paths free of tripping hazards and handicap accessible |
|  | Spectator Bleachers Municipality does not own this equipment □ |
| 29 |  |  |  | Are bleachers on grass or a concrete - if on hard surface, should have fall guards |
| 30 |  |  |  | Are there more than three levels of benches - less than 3 guard rails are not required |
| 31 |  |  |  | If yes, is back & side fall protection provided on areas above 30” Is it at least 42” tall |
| 31 |  |  |  | Do openings in rails or fences restrict the ability to climb or gain a toe hold |
| 32 |  |  |  | Are the bleachers structurally sound & appear to be in good condition |
| 33 |  |  |  | Have 4 seat or more bleachers been inspected by a PE within the last 2 years |