|  |
| --- |
| Beach, Boardwalk & Bike Path Facilities Hazard Identification Inspection |
| Agency: | Inspection Date: |
| Name of Inspector: | Title: |
| Location Inspected: |
| # | Needs Work | N/A | OK | Condition Surveyed |
|  | Boardwalks |
| 1 |  |  |  | Are handrails on entrance ramps in good repair |
| 2 |  |  |  | Is there a guardrail on all exposed edges? |
| 3 |  |  |  | Does the guardrail have a top rail between 44-48 inches? |
| 4 |  |  |  | Is there a mid-rail and infill to the deck below? |
| 5 |  |  |  | Is the spacing between boards less than 1/8 th inch? |
| 6 |  |  |  | Are there any cracked or broken boards? |
| 7 |  |  |  | Are bicycle riding times posted? And enforced? |
| 8 |  |  |  | Are benches, handrails and walking surfaces free of splinters? |
| 9 |  |  |  | Are there sufficient waste receptacles? |
| 10 |  |  |  | Are skateboarding and rollerblading prohibited? |
| 11 |  |  |  | Are pets prohibited or rules posted? |
|  | Bike Paths |
| 12 |  |  |  | Paving surface in good condition free of ruts, holes & broken edges |
| 13 |  |  |  | Clearance from surface to 7” height throughout travel area |
| 14 |  |  |  | Stop signs at road crossings |
| 15 |  |  |  | Bike racks and locking stations at tourist stops? |
| 16 |  |  |  | Rules posted, i.e., Helmets required, speed limits? Skateboards? |
| 17 |  |  |  | Are paths accessible to the handicapped and pedestrians? |
| 18 |  |  |  | Is lighting provided, is it operational |
| 19 |  |  |  | Is vegetation trimmed back at least 5 feet on sides to aid visibility |
| 20 |  |  |  | Are there methods to call for help? Voice or phone boxes? |
| 21 |  |  |  | Are restrooms or rest areas provided? Are they maintained? |
| 22 |  |  |  | Is there a refuse collection system? Trash cans? Are they serviced? |
|  | Beaches and Lakefronts |
| 23 |  |  |  | Any known hazards in the vicinity are safeguarded & posted? |
| 24 |  |  |  | All waterfront rules & restrictions are posted? i.e. no alcohol |
| 25 |  |  |  | Bather rules & policies are posted? |
| 26 |  |  |  | Beaches are maintained free of recognized hazards? i.e. broken glass |
| 27 |  |  |  | At least one LG stand for every 300 foot of designated bathing area? |
| 28 |  |  |  | 600 foot of ¼ inch poly line with brass swivel snap hook? |
| 29 |  |  |  | One Ring Buoy 18 inches in diameter with 75 foot of ¼ inch line? |
| 30 |  |  |  | Skating surfaces free of significant cracks. Attractions are in good condition. |
| 31 |  |  |  | Bathrooms are clean, supplies adequate, and trash emptied |
| 32 |  |  |  | Concession stands are structurally sound and secured from unauthorized use. |