|  |
| --- |
| Police DepartmentFacilities Hazard Identification Inspection |
| Agency: | Inspection Date: |
| Name of Inspector: | Title: |
| Location Inspected: |
| # | Needs Work | N/A | OK | Condition Surveyed |
|  | Exterior Grounds, Walkways and Parking Areas |
| 1 |  |  |  | Exterior lighting of grounds, walkways, & parking areas adequate and operational |
| 2 |  |  |  | Parking lots and driveways free of significant cracks and water accumulation |
| 3 |  |  |  | Sidewalks and stairs / ramps free of significant trip or slip hazards |
| 4 |  |  |  | Rails and handrails are present, not loose, and in good condition |
| 5 |  |  |  | Roofs, gutters, and downspouts are clean and control run-off properly |
| 6 |  |  |  | The area is free of signs of rodent, insects, or feral animals being present |
|  | Life Safety and Fire Protection Equipment |
| 7 |  |  |  | Intrusion alarm is operational and free of trouble or active alarms |
| 8 |  |  |  | Closed-circuit TV cameras are operational, properly aimed and focused |
| 9 |  |  |  | Fire sprinkler system is operational, controls valve accessible & locked / alarmed |
| 10 |  |  |  | Fire detection system operational and free of trouble or active alarms |
| 11 |  |  |  | Fire extinguishers are accessible and in good condition – SIGN REAR OF TAGS |
| 12 |  |  |  | Emergency and Exit lights are lit and worked when test button/switch used |
| 13 |  |  |  | Panic hardware on exit doors worked easily. Doors latched when closing |
| 14 |  |  |  | Emergency generator operated on weekly basis |
| 15 |  |  |  | First aid kit fully stocked. AED in READY condition. Expirations dates checked |
| 16 |  |  |  | Panic alarms tested and received at monitoring station |
|  | Building, Housekeeping, and Sanitary Conditions |
| 17 |  |  |  | Sally port overhead doors entrapment sensors tested and operated properly |
| 18 |  |  |  | Sally port floors are clean and clear of clutter. The area is free of potential weapons. |
| 19 |  |  |  | Dispatch Area-electrical and communication wires are orderly & not a trip hazard |
| 20 |  |  |  | Fitness Area equipment is in good condition and stored not to present trip hazard |
| 21 |  |  |  | Locker Rooms-showers, counters, and floors are clean. Personal items secured |
| 22 |  |  |  | No unapproved space heaters or extension cords are present |
| 23 |  |  |  | Approved space heaters are clear of combustible materials |
| 24 |  |  |  | Electrical cords are not secured to furniture, through doors, or across paths of travel |
| 25 |  |  |  | Hallways / stairwells are well-lit, clear of obstructions and free of slip-trip hazards |
| 26 |  |  |  | Stair treads and railing / handrail are secure. |
| 27 |  |  |  | Areas around and 36” in front of electrical panels is clear |
| 28 |  |  |  | Areas and floor around mechanical equipment is free of slip-trip hazards. |
| 29 |  |  |  | Storage is 18” below sprinkler heads or 24” below ceiling |
|  | Building, Housekeeping, and Sanitary Conditions (cont.) |
| 30 |  |  |  | No storage in HVAC and other mechanical rooms. Tools & equipment orderly. |
| 31 |  |  |  | Storage areas of cleaning & hazardous substances clean, organized, & labeled |
| 32 |  |  |  | Electrical cords of office and kitchen machines are in good condition & orderly |
| 33 |  |  |  | Trash is emptied. Housekeeping is adequate |
| 34 |  |  |  | Bathrooms are clean, supplies adequate, and trash emptied |
| 35 |  |  |  | The refrigerator and stove are clean. Kitchen is free of signs of rodents / insects. |
| 36 |  |  |  | Coffee pots, microwave, and kitchen appliances are clean and cords intact |
| 37 |  |  |  | Walls, floors, and ceilings are free of water, rodent, or mechanical damage. |