|  |
| --- |
| Vacant Housing UnitFacilities Hazard Identification Inspection |
| Agency: | Inspection Date: |
| Name of Inspector: | Title: |
| Location Inspected: |
| # | Needs Work | N/A | OK | Condition Surveyed |
|  | Exterior Areas |
| 1 |  |  |  | Exterior vegetation does not create an obstacle to security of the unit |
| 2 |  |  |  | Exterior vegetation does not obstruct fire department operations |
| 3 |  |  |  | Exterior windows and security features are in good condition and properly secured |
| 4 |  |  |  | Exterior of unit is free of excessive litter or debris |
| 5 |  |  |  | Roof, gutters, and downspouts are clean and control run-off properly |
| 6 |  |  |  | Area is free of signs of rodent, insects, or feral animals being present |
| **Comments:** |
|  | Building, Housekeeping and Sanitary Conditions |
| 7 |  |  |  | Entry door to unit opens fully and closes securely |
| 8 |  |  |  | Entry door to unit lock or locks work properly. |
| 9 |  |  |  | Unit is generally in good condition with no signs of vandalism or destruction. |
| 10 |  |  |  | All windows are locked |
| 11 |  |  |  | Fire extinguisher is present, mounted, and in good condition |
| 12 |  |  |  | Outlets, switches, and electrical junction boxes are covered – no exposed wiring |
| 13 |  |  |  | Smoke and carbon monoxide detectors are present and work when test button used |
| 14 |  |  |  | Kitchen suppression system is in proper working order. |
| 15 |  |  |  | Heating system is working properly and thermostat set at \_\_\_\_\_ ℉ |
| 16 |  |  |  | HVAC closet is clear of storage and equipment is free of obvious damage |
| 17 |  |  |  | Unit is free of signs of rodent infestation, including dropping and holes |
| 18 |  |  |  | Unit is free of signs of insect infestation |
| 19 |  |  |  | Kitchen cabinets are empty of food and cleaned |
| 20 |  |  |  | Unit is free of obvious damage or vandalism |
| 21 |  |  |  | Unit is generally clean. |
| **Comments:** |
|  | Check for Visible Signs of Water Leaks |
|  |  |  |  | Under kitchen and bathroom sinks. Run water and check for leaks. |
| 22 |  |  |  | Around refrigerator |
| 23 |  |  |  | Around windows and air conditioners |
| 24 |  |  |  | Around toilet. Flush and check for leaks and proper water shut-off |
| 25 |  |  |  | The unit is free of visible mold throughout.  |
| 26 |  |  |  | The unit does not smell of must or mold. |
| 27 |  |  |  | Ceiling tiles are free of water stains. |
| **Comments:** |

\* Consider shutting off utilities to the unit